-------------------------------------------------------------------------------------------------------------------
INSTALL
-------------------------------------------------------------------------------------------------------------------
   You need to prepare the documents:
		ds2Linux
		Dingux Z4 (or Dingux Z5) system files(other Dingux versions were not tested, maybe you can try).
		DSTWO system files (DSTWO official release).

		NOTE:In the following use Dingux XX instead of Dingux Z4 (or Dingux Z5,or other Dingux version).

  1. Check whether your memory card is FAT32 format, first use, we recommend a full format, then enter the following installation steps.

  2. Firstly, copy rootfs (from Dingux XX) to your memory card.

  3. And then copy zImage_DS2 (from ds2Linux) to your memory card.

  4. After confirm the above files are copied, copy the folders of LOCAL, GAME
     (from Dingux XX, other dingux XX system files are useless to ds2Linux) to your memory card completely.

  5. Copy DSTWO system folder _dstwo (DSTWO official release) to your memory card.

  6. Copy the folder of _dstwoplug which contains four files (dstwoLinux.plg, dstwoLinux.ini, dstwoLinux.bmp and
     ds2Linux_boot.bmp) to your memory card.

     At this point, all files have been installed, you can immediately start using.
     Enjoy yourself!


-------------------------------------------------------------------------------------------------------------------
ds2Linux function key
-------------------------------------------------------------------------------------------------------------------
	START + L: switch display mode
	START + LEFT/RIGHT: move x coordinate in display mode of the original size.
	START + UP/DOWN: move y coordinate in display mode of the original size.
	START + R: exit ds2Linux plug then return to ds2 main interface.

	NOTE:Maybe these function keys conflict with simulator shortcuts.
