fulldump: dumps OS 4MiB NOR to root at /dump.bin

fullerase: erases full 4MiB NOR

fullrestore: expects a 4MiB file (exactly - be warned there is no error handling) called "ez4.bin" to bin the root of your slot1 card,
	it erases the entire chip, then writes the contents to the OS NOR chip
	
proper dldi patching required if your slot1 kernel doesn't support autopatch for dump or restore functions.
