## ColorBars / ColorBarsHD

`ColorBars` (int "width", int "height", string "pixel_type")

The `ColorBars` filter produces a video clip containing SMPTE color bars (Rec. ITU-R BT.801-1) scaled to any image size. By default, a clip is produced of 640x480, RGB32 [16,235], 29.97 fps, 1 hour long, alpha channel opaque.
The `ColorBarsHD` filter (added in v2.60) produces a video clip containing SMPTE color bars (Rec. ITU-R BT.709 / arib std b28 v1.0) scaled to any image size. By default, a clip is produced of 1288x720, YV24, 29.97 fps, 1 hour long.

For both filters, a test tone is also generated. Test tone is a 440Hz sine at 48KHz, 16 bit, stereo. The tone pulses in the RIGHT speaker, being turned on and off once every second.

For ColorBars the following pixel types are supported: "YUY2" (v2.56), "YV12" (v2.56), "YV24" (v2.60), or (default) "RGB32". For ColorsBarsHD only "YV24" is supported.

Note, that for example

    ColorBars(pixel_type="YUY2")

is almost equivalent with (the -I and +Q patterns have Y increased to the minimum legal value for RGB)

    ColorBars(pixel_type="RGB32")
    ConvertToYUY2(matrix="PC.601")  # doesn't scale the luma range

When directly generating YUV format data the color transitions are arranged to occur on a chroma aligned boundary.

The lower part of ColorBars is called the pluge. From left to right it consists of: -I, white, +Q, black, -4/0/+4 IRE levels and black. The -4/0/4 IRE levels can be used to set the brightness correctly. The -4 IRE and 0 IRE should have the same brightness, and the +4 IRE should be a little brighter than -4/0 IRE. The -I/+Q levels are not really interesting, since they are not used anymore for NTSC (analog TV), but they were used to set the chrominance correctly. More information about the colorbars and the pluge can be found here.

Changes:

v2.56 | Added pixel_type="YUY2"/"YV12".
v2.60 | Added pixel_type="YV24" to ColorBars. Initial release of ColorBarsHD.

`$Date: 2011/04/17 03:58:18 $`